VTNET(4)

NAME
vtnet - VirtIO Ethernet driver

SYNOPSIS
To compile this driver into the kernel, place the following lines in your kernel configuration file:

device vtnet

Alternatively, to load the driver as a module at boot time, place the following line in loader.conf(5):

    if_vtnet_load="YES"

DESCRIPTION
The vtnet device driver provides support for VirtIO Ethernet devices.

If the hypervisor advertises the appropriate features, the vtnet driver supports TCP/UDP checksum offload for both transmit and receive, TCP segmentation offload (TSO), TCP large receive offload (LRO), hardware VLAN tag stripping/insertion features, a multicast hash filter, as well as Jumbo Frames (up to 9216 bytes), which can be configured via the interface MTU setting.

Two flavors of TCP LRO are supported: Hardware TCP LRO, which is performed by the host providing TCP segments larger than the MTU to the guest, and Software TCP LRO, which is performed by the network stack of the guest processing TCP segments in an optimized way. Only one flavour of TCP LRO should be used. Since hardware TCP LRO can have bad interactions with IP forwarding and software TCP LRO mitigates several drawbacks of hardware TCP LRO, the default setting is to disable hardware TCP LRO. See the loader tunable hw.vtnet.X.lro_disable.

TCP/UDP receive checksum offload cannot be configured independently for IPv4 and IPv6. Selecting an MTU larger than 1500 bytes with the ifconfig(8) utility configures the adapter to receive and transmit Jumbo Frames.

For more information on configuring this device, see ifconfig(8).

LOADER TUNABLES
Tunables can be set at the loader(8) prompt before booting the kernel or stored in loader.conf(5).

hw.vtnet.csum_disable

hw.vtnet.X.csum_disable
    This tunable disables receive and transmit checksum offloading for TCP and UDP. This also implies that TCP segmentation offloading and large receive offload are disabled. The default value is 0.

hw.vtnet.tso_disable

hw.vtnet.X.tso_disable
    This tunable disables TCP segmentation offloading. The default value is 0.

hw.vtnet.lro_disable

hw.vtnet.X.lro_disable
    This tunable disables hardware TCP LRO. The default value is 1.

hw.vtnet.mq_disable

hw.vtnet.X.mq_disable
    This tunable disables multiqueue. The default value is 0.

hw.vtnet.mq_max_pairs

hw.vtnet.X.mq_max_pairs
    This tunable sets the maximum number of transmit and receive queue pairs. Multiple queues are only supported when the Multiqueue feature is negotiated. This driver supports a maximum of 8 queue pairs. The number of queue pairs used is the lesser of the maximum supported by the driver and the hypervisor, the number of CPUs present in the guest, and this tunable if not zero. The default value is 0.

hw.vtnet.tso_maxlen

hw.vtnet.X.tso_maxlen
    This tunable sets the TSO burst limit. The default value is 65535.

hw.vtnet.rx_process_limit

hw.vtnet.X.rx_process_limit
    This tunable sets the number of RX segments processed in one pass. The default value is 1024.

hw.vtnet.lro_entry_count

hw.vtnet.X.lro_entry_count
    This tunable sets the software TCP LRO entry count. The default value is 128, the minimum value is 8.

hw.vtnet.lro_mbufq_depth

hw.vtnet.X.lro_mbufq_depth
    This tunable sets the depth of the software TCP LRO mbuf queue. The default value is 0.

hw.vtnet.altq_disable
    This tunable disables ALTQ support, allowing the use of multiqueue instead. This option applies to all interfaces. The default value is 0.

TRANSMIT QUEUE STATISTICS
For each transmit queue of each interface the following read-only statistics are provided:

dev.vtnet.X.txqY.rescheduled
    The number of times the transmit interrupt handler was rescheduled.

dev.vtnet.X.txqY.tso
    The number of times TCP segment offloading was performed.

dev.vtnet.X.txqY.csum
    The number of times transmit checksum offloading for UDP or TCP was performed.

dev.vtnet.X.txqY.omcasts
    The number of multicast packets that were transmitted.

dev.vtnet.X.txqY.obytes
    The number of bytes that were transmitted (based on Ethernet frames).

dev.vtnet.X.txqY.opackets
    The number of packets that were transmitted (Ethernet frames).

RECEIVE QUEUE STATISTICS
For each receive queue of each interface the following read-only statistics are provided:

dev.vtnet.X.rxqY.rescheduled
    The number of times the receive interrupt handler was rescheduled.

dev.vtnet.X.rxqY.host_lro
    The number of times TCP large receive offload was performed.

dev.vtnet.X.rxqY.csum_failed
    The number of times a packet with a request for receive or transmit checksum offloading was received and this request failed. The different reasons for the failure are counted by dev.vtnet.X.rx_csum_inaccessible_ipproto, dev.vtnet.X.rx_csum_bad_ipproto, and dev.vtnet.X.rx_csum_bad_ethtype.

dev.vtnet.X.rxqY.csum
    The number of times receive checksum offloading for UDP or TCP was performed.

dev.vtnet.X.rxqY.ierrors
    The number of times an error occurred during input processing.

dev.vtnet.X.rxqY.iqdrops
    The number of times a packet was dropped during input processing.

dev.vtnet.X.rxqY.ibytes
    The number of bytes that were received (based on Ethernet frames).

dev.vtnet.X.rxqY.ipackets
    The number of packets that were received (Ethernet frames).

INTERFACE TRANSMIT STATISTICS
For each interface the following read-only transmit statistics are provided:

dev.vtnet.X.tx_task_rescheduled
    The sum of dev.vtnet.X.txqY.rescheduled over all transmit queues of the interface.

dev.vtnet.X.tx_tso_offloaded
    The sum of dev.vtnet.X.txqY.tso over all transmit queues of the interface.

dev.vtnet.X.tx_csum_offloaded
    The sum of dev.vtnet.X.txqY.csum over all transmit queues of the interface.

dev.vtnet.X.tx_defrag_failed
    The number of times an attempt to defragment an mbuf chain failed during a transmit operation.

dev.vtnet.X.tx_defragged
    The number of times an mbuf chain was defragmented during a transmit operation.

dev.vtnet.X.tx_tso_without_csum
    The number of times TCP segment offloading was attempted without transmit checksum offloading.

dev.vtnet.X.tx_tso_not_tcp
    The number of times TCP segment offloading was attempted for a non-TCP packet.

dev.vtnet.X.tx_csum_proto_mismatch
    The number of times the IP protocol version of the transmit checksum offloading request did not match the IP protocol version of the packet.

dev.vtnet.X.tx_csum_unknown_ethtype
    The number of times a transmit offload operation was requested for an ethernet frame for which the EtherType was neither IPv4 nor IPv6 (considering simple VLAN tagging).

INTERFACE RECEIVE STATISTICS
For each interface the following read-only receive statistics are provided:

dev.vtnet.X.rx_task_rescheduled
    The sum of dev.vtnet.X.rxqY.rescheduled over all receive queues of the interface.

dev.vtnet.X.rx_csum_offloaded
    The sum of dev.vtnet.X.rxqY.csum over all receive queues of the interface.

dev.vtnet.X.rx_csum_failed
    The sum of dev.vtnet.X.rxqY.csum_failed over all receive queues of the interface.

dev.vtnet.X.rx_csum_inaccessible_ipproto
    The number of times a packet with a request for receive or transmit checksum offloading was received where the IP protocol was not accessible.

dev.vtnet.X.rx_csum_bad_ipproto
    The number of times a packet with a request for receive or transmit checksum offloading was received where the IP protocol was neither TCP nor UDP.

dev.vtnet.X.rx_csum_bad_ethtype
    The number of times a packet with a request for receive or transmit checksum offloading was received where the EtherType was neither IPv4 nor IPv6.

dev.vtnet.X.rx_mergeable_failed
    The number of times receiving a mergable buffer failed.

dev.vtnet.X.rx_enq_replacement_failed
    The number of times the enqueuing the replacement receive mbuf chain failed.

dev.vtnet.X.rx_frame_too_large
    The number of times the frame was loger than the mbuf chain during large receive offload without mergeable buffers.

dev.vtnet.X.mbuf_alloc_failed
    The number of times an mbuf cluster allocation for the receive buffer failed.

INTERFACE CONFIGURATION PARAMETER
For each interface the following read-only configuration parameters are provided:

dev.vtnet.X.act_vq_pairs
    The number of active virtqueue pairs.

dev.vtnet.X.req_vq_pairs
    The number of requested virtqueue pairs.

dev.vtnet.X.max_vq_pairs
    The maximum number of supported virtqueue pairs.

dev.vtnet.X.flags
    The flags of the interface. Mostly for debugging purposes.

dev.vtnet.X.features
    The features of the interface as defined by the virtio specification.

SEE ALSO
arp(4), netintro(4), ng_ether(4), virtio(4), vlan(4), ifconfig(8)

HISTORY
The vtnet driver was written by Bryan Venteicher <bryanv@FreeBSD.org>. It first appeared in FreeBSD 9.0.

CAVEATS
The vtnet driver only supports LRO when the hypervisor advertises the mergeable buffer feature.