BUS_ALLOC_RESOURCE(9)

NAME
bus_alloc_resource, bus_alloc_resource_any, bus_alloc_resource_anywhere - allocate resources from a parent bus

SYNOPSIS
#include <sys/param.h>
#include <sys/bus.h>

#include <machine/bus.h>
#include <sys/rman.h>
#include <machine/resource.h>
struct resource *
bus_alloc_resource(device_t dev, int type, int rid, rman_res_t start, rman_res_t end, rman_res_t count, u_int flags);
struct resource *
bus_alloc_resource_any(device_t dev, int type, int rid, u_int flags);
struct resource *
bus_alloc_resource_anywhere(device_t dev, int type, int rid, rman_res_t count, u_int flags);

DESCRIPTION
This is an easy interface to the resource-management functions. It hides the indirection through the parent's method table. This function generally should be called in attach, but (except in some rare cases) never earlier.

The bus_alloc_resource_any() and bus_alloc_resource_anywhere() functions are convenience wrappers for bus_alloc_resource(). bus_alloc_resource_any() sets start, end, and count to the default resource (see description of start below). bus_alloc_resource_anywhere() sets start and end to the default resource and uses the provided count argument.

The arguments are as follows:

dev is the device that requests ownership of the resource. Before allocation, the resource is owned by the parent bus.

type is the type of resource you want to allocate. It is one of:

PCI_RES_BUS
    for PCI bus numbers

SYS_RES_IRQ
    for IRQs

SYS_RES_DRQ
    for ISA DMA lines

SYS_RES_IOPORT
    for I/O ports

SYS_RES_MEMORY
    for I/O memory

rid is a bus specific handle that identifies the resource being allocated. For ISA this is an index into an array of resources that have been setup for this device by either the PnP mechanism, or via the hints mechanism. For PCCARD, this is an index into the array of resources described by the PC Card's CIS entry. For PCI, the offset into PCI config space which has the BAR to use to access the resource.

start and end are the start/end addresses of the resource. If you specify values of 0ul for start and ~0ul for end and 1 for count, the default values for the bus are calculated.

count is the size of the resource. For example, the size of an I/O port is usually 1 byte (but some devices override this). If you specified the default values for start and end, then the default value of the bus is used if count is smaller than the default value and count is used, if it is bigger than the default value.

flags sets the flags for the resource. You can set zero or more of these flags:

RF_ACTIVE
    activate resource atomically.

RF_PREFETCHABLE
    resource is prefetchable.

RF_SHAREABLE
    resource permits contemporaneous sharing. It should always be set unless you know that the resource cannot be shared. It is the bus driver's task to filter out the flag if the bus does not support sharing.

RF_UNMAPPED
    do not establish implicit mapping when activated via bus_activate_resource(9).

RETURN VALUES
A pointer to struct resource is returned on success, a null pointer otherwise.

EXAMPLES
This is some example code that allocates a 32 byte I/O port range and an IRQ.

    	struct resource *portres, *irqres;
    	portres = bus_alloc_resource(dev, SYS_RES_IOPORT, 0,
    			0ul, ~0ul, 32, RF_ACTIVE);
    	irqres = bus_alloc_resource_any(dev, SYS_RES_IRQ, 0,
    			RF_ACTIVE | RF_SHAREABLE);

SEE ALSO
bus_activate_resource(9), bus_adjust_resource(9), bus_map_resource(9), bus_release_resource(9), device(9), driver(9)

AUTHORS
-nosplit This manual page was written by Alexander Langer <alex@big.endian.de> with parts by Warner Losh <imp@FreeBSD.org>.