fdt_pinctrl(9)

NAME
fdt_pinctrl - helper functions for FDT pinmux controller drivers

SYNOPSIS
#include <dev/fdt/fdt_pinctrl.h>
int
fdt_pinctrl_configure(device_t client, u_int index);
int
fdt_pinctrl_configure_by_name(device_t client, const char * name);
int
fdt_pinctrl_register(device_t pinctrl, const char *pinprop);
int
fdt_pinctrl_configure_tree(device_t pinctrl);

DESCRIPTION
fdt_pinctrl(4) provides an API for manipulating I/O pin configurations on pinmux controllers and pinmux clients. On the controller side, the standard newbus probe and attach methods are implemented. As part of handling attach, it calls the fdt_pinctrl_register() function to register itself as a pinmux controller. Then fdt_pinctrl_configure_tree() is used to walk the device tree and configure pins specified by the pinctrl-0 property for all active devices. The driver also implements the fdt_pinctrl_configure() method, which allows client devices to change their pin configurations after startup. If a client device requires a pin configuration change at some point of its lifecycle, it uses the fdt_pinctrl_configure() or fdt_pinctrl_configure_by_name() functions.

fdt_pinctrl_configure() is used by client device client to request a pin configuration described by the pinctrl-N property with index index.

fdt_pinctrl_configure_by_name() is used by client device client to request the pin configuration with name name.

fdt_pinctrl_register() registers a pinctrl driver so that it can be used by other devices which call fdt_pinctrl_configure() or fdt_pinctrl_configure_by_name(). It also registers each child node of the pinctrl driver's node which contains a property with the name given in pinprop. If pinprop is NULL, every descendant node is registered. It is possible for the driver to register itself as a pinmux controller for more than one pin property type by calling fdt_pinctrl_register() multiple types.

fdt_pinctrl_configure_tree() walks through enabled devices in the device tree. If the pinctrl-0 property contains references to child nodes of the specified pinctrl device, their pins are configured.

EXAMPLES

    static int
    foo_configure_pins(device_t dev, phandle_t cfgxref)
    {
    	phandle_t cfgnode;
    	uint32_t *pins, *functions;
    	int npins, nfunctions;
    	cfgnode = OF_node_from_xref(cfgxref);
    	pins = NULL;
    	npins = OF_getencprop_alloc_multi(cfgnode, "foo,pins", sizeof(*pins),
    	    (void **)&pins);
    	functions = NULL;
    	nfunctions = OF_getencprop_alloc_multi(cfgnode, "foo,functions",
    	    sizeof(*functions), (void **)&functions);
    	...
    }
    static int
    foo_is_gpio(device_t dev, device_t gpiodev, bool *is_gpio)
    {
    	return (foo_is_pin_func_gpio(is_gpio));
    }
    static int
    foo_set_flags(device_t dev, device_t gpiodev, uint32_t pin, uint32_t flags)
    {
    	int rv;
    	rv = foo_is_pin_func_gpio(is_gpio);
    	if (rv != 0)
    		return (rv);
    	foo_set_flags(pin, flags);
    	return (0);
    }
    static int
    foo_get_flags(device_t dev, device_t gpiodev, uint32_t pin, uint32_t *flags)
    {
    	int rv;
    	rv = foo_is_pin_func_gpio(is_gpio);
    	if (rv != 0)
    		return (rv);
    	foo_get_flags(pin, flags);
    	return (0);
    }
    static int
    foo_attach(device_t dev)
    {
    	...
    	fdt_pinctrl_register(dev, "foo,pins");
    	/*
    	 * It is possible to register more than one pinprop handler
    	 */
    	fdt_pinctrl_register(dev, "bar,pins");
    	fdt_pinctrl_configure_tree(dev);
    	return (0);
    }
    static device_method_t foo_methods[] = {
    	...
    	/* fdt_pinctrl interface */
    	DEVMETHOD(fdt_pinctrl_configure, foo_configure_pins),
    	DEVMETHOD(fdt_pinctrl_is_gpio, foo_is_gpio),
    	DEVMETHOD(fdt_pinctrl_set_flags, foo_set_flags),
    	DEVMETHOD(fdt_pinctrl_get_flags, foo_get_flags),
    	/* Terminate method list */
    	DEVMETHOD_END
    };
    DRIVER_MODULE(foo, simplebus, foo_driver, foo_devclass, NULL, NULL);

SEE ALSO
fdt_pinctrl(4)

AUTHORS
This manual page was written by Oleksandr Tymoshenko.