PF(4)

NAME
pf - packet filter

SYNOPSIS
device pf
options PF_DEFAULT_TO_DROP

In rc.conf(5):
pf_enable="YES"

In loader.conf(5):
net.pf.states_hashsize
net.pf.source_nodes_hashsize
net.pf.rule_tag_hashsize
net.pf.udpendpoint_hashsize
net.pf.default_to_drop

In sysctl.conf(5):
net.pf.request_maxcount
net.pf.filter_local

DESCRIPTION
Packet filtering takes place in the kernel. A pseudo-device, /dev/pf, allows userland processes to control the behavior of the packet filter through an ioctl(2) interface. There are commands to enable and disable the filter, load rulesets, add and remove individual rules or state table entries, and retrieve statistics. The most commonly used functions are covered by pfctl(8).

Manipulations like loading a ruleset that involve more than a single ioctl(2) call require a so-called ticket, which prevents the occurrence of multiple concurrent manipulations.

Fields of ioctl(2) parameter structures that refer to packet data (like addresses and ports) are generally expected in network byte-order.

Rules and address tables are contained in so-called anchors. When servicing an ioctl(2) request, if the anchor field of the argument structure is empty, the kernel will use the default anchor (i.e., the main ruleset) in operations. Anchors are specified by name and may be nested, with components separated by ‘/’ characters, similar to how file system hierarchies are laid out. The final component of the anchor path is the anchor under which operations will be performed.

SYSCTL VARIABLES
The following variables can be entered at the loader(8) prompt, set in loader.conf(5), sysctl.conf(5), or changed at runtime with sysctl(8):

net.pf.filter_local
    This tells pf to also filter on the loopback output hook. This is typically used to allow redirect rules to adjust the source address.

net.pf.request_maxcount
    The maximum number of items in a single ioctl call.

LOADER TUNABLES
The following tunables can be entered at the loader(8) prompt, or set in loader.conf(5):

net.pf.states_hashsize
    Size of hash table that stores states. Should be power of 2. Default value is 131072.

net.pf.source_nodes_hashsize
    Size of hash table that stores source nodes. Should be power of 2. Default value is 32768.

net.pf.rule_tag_hashsize
    Size of the hash table that stores tags.

net.pf.udpendpoint_hashsize
    Size of hash table that store UDP endpoint mappings. Should be power of 2. Default value is 32768.

net.pf.default_to_drop
    This value overrides options PF_DEFAULT_TO_DROP from kernel configuration file.

net.pf.filter_local
    This tells pf to also filter on the loopback output hook. This is typically used to allow redirect rules to adjust the source address.

net.pf.request_maxcount
    The maximum number of items in a single ioctl call.

Read only sysctl(8) variables with matching names are provided to obtain current values at runtime.

KERNEL OPTIONS
The following options in the kernel configuration file are related to pf operation:

PF_DEFAULT_TO_DROP
    Change default policy to drop by default

IOCTL INTERFACE
pf supports the following ioctl(2) commands, available through <net/pfvar.h>:

DIOCSTART
    Start the packet filter.

DIOCSTOP
    Stop the packet filter.

DIOCSTARTALTQ
    Start the ALTQ bandwidth control system (see altq(9)).

DIOCSTOPALTQ
    Stop the ALTQ bandwidth control system.

DIOCBEGINADDRS struct pfioc_pooladdr *pp

        struct pfioc_pooladdr {
        	u_int32_t		action;
        	u_int32_t		ticket;
        	u_int32_t		nr;
        	u_int32_t		r_num;
        	u_int8_t		r_action;
        	u_int8_t		r_last;
        	u_int8_t		af;
        	char			anchor[MAXPATHLEN];
        	struct pf_pooladdr	addr;
        };

    Clear the buffer address pool and get a ticket for subsequent DIOCADDADDR, DIOCADDRULE, and DIOCCHANGERULE calls.

DIOCADDADDR struct pfioc_pooladdr *pp

    Add the pool address addr to the buffer address pool to be used in the following DIOCADDRULE or DIOCCHANGERULE call. All other members of the structure are ignored.

DIOCADDRULE struct pfioc_rule *pr

        struct pfioc_rule {
        	u_int32_t	action;
        	u_int32_t	ticket;
        	u_int32_t	pool_ticket;
        	u_int32_t	nr;
        	char		anchor[MAXPATHLEN];
        	char		anchor_call[MAXPATHLEN];
        	struct pf_rule	rule;
        };

    Add rule at the end of the inactive ruleset. This call requires a ticket obtained through a preceding DIOCXBEGIN call and a pool_ticket obtained through a DIOCBEGINADDRS call. DIOCADDADDR must also be called if any pool addresses are required. The optional anchor name indicates the anchor in which to append the rule. nr and action are ignored.

DIOCADDALTQ struct pfioc_altq *pa
    Add an ALTQ discipline or queue.

        struct pfioc_altq {
        	u_int32_t	action;
        	u_int32_t	ticket;
        	u_int32_t	nr;
        	struct pf_altq  altq;
        };

DIOCGETRULES struct pfioc_rule *pr
    Get a ticket for subsequent DIOCGETRULE calls and the number nr of rules in the active ruleset.

DIOCGETRULE struct pfioc_rule *pr
    Get a rule by its number nr using the ticket obtained through a preceding DIOCGETRULES call. If action is set to PF_GET_CLR_CNTR, the per-rule statistics on the requested rule are cleared.

DIOCGETADDRS struct pfioc_pooladdr *pp
    Get a ticket for subsequent DIOCGETADDR calls and the number nr of pool addresses in the rule specified with r_action, r_num, and anchor.

DIOCGETADDR struct pfioc_pooladdr *pp
    Get the pool address addr by its number nr from the rule specified with r_action, r_num, and anchor using the ticket obtained through a preceding DIOCGETADDRS call.

DIOCGETALTQS struct pfioc_altq *pa
    Get a ticket for subsequent DIOCGETALTQ calls and the number nr of queues in the active list.

DIOCGETALTQ struct pfioc_altq *pa
    Get the queueing discipline altq by its number nr using the ticket obtained through a preceding DIOCGETALTQS call.

DIOCGETQSTATS struct pfioc_qstats *pq
    Get the statistics on a queue.

        struct pfioc_qstats {
        	u_int32_t	 ticket;
        	u_int32_t	 nr;
        	void		*buf;
        	int		 nbytes;
        	u_int8_t	 scheduler;
        };

    This call fills in a pointer to the buffer of statistics buf, of length nbytes, for the queue specified by nr.

DIOCGETRULESETS struct pfioc_ruleset *pr

        struct pfioc_ruleset {
        	u_int32_t	 nr;
        	char		 path[MAXPATHLEN];
        	char		 name[PF_ANCHOR_NAME_SIZE];
        };

    Get the number nr of rulesets (i.e., anchors) directly attached to the anchor named by path for use in subsequent DIOCGETRULESET calls. Nested anchors, since they are not directly attached to the given anchor, will not be included. This ioctl returns ENOENT if the parent anchor given at path does not exist.

DIOCGETRULESET struct pfioc_ruleset *pr
    Get a ruleset (i.e., an anchor) name by its number nr from the given anchor path, the maximum number of which can be obtained from a preceding DIOCGETRULESETS call. This ioctl returns ENOENT if the parent anchor given by path does not exist or EBUSY if the index passed in by nr is greater than the number of anchors.

DIOCADDSTATE struct pfioc_state *ps
    Add a state entry.

        struct pfioc_state {
        	struct pfsync_state	state;
        };

DIOCGETSTATENV struct pfioc_nv *nv
    Extract the entry identified by the id and creatorid fields of the state nvlist from the state table.

DIOCKILLSTATESNV struct pfioc_nv nv
    Remove matching entries from the state table. This ioctl returns the number of killed states in killed.

        nvlist pf_state_cmp {
        	number			id;
        	number			creatorid;
        	number			direction;
        };
        nvlist pf_kill {
        	nvlist pf_state_cmp	cmp;
        	number			af;
        	number			proto;
        	nvlist pf_rule_addr	src;
        	nvlist pf_rule_addr	dst;
        	string			ifname[IFNAMSIZ];
        	string			label[PF_RULE_LABEL_SIZE];
        };

DIOCCLRSTATESNV struct pfioc_nv nv
    Clear all states. It works like DIOCKILLSTATESNV, but ignores the af, proto, src, and dst fields of the pf_kill nvlist.

DIOCSETSTATUSIF struct pfioc_if *pi
    Specify the interface for which statistics are accumulated.

        struct pfioc_if {
        	char		 ifname[IFNAMSIZ];
        };

DIOCGETSTATUS struct pf_status *s
    Get the internal packet filter statistics.

        struct pf_status {
        	u_int64_t	counters[PFRES_MAX];
        	u_int64_t	lcounters[LCNT_MAX];
        	u_int64_t	fcounters[FCNT_MAX];
        	u_int64_t	scounters[SCNT_MAX];
        	u_int64_t	pcounters[2][2][3];
        	u_int64_t	bcounters[2][2];
        	u_int32_t	running;
        	u_int32_t	states;
        	u_int32_t	src_nodes;
        	u_int32_t	since;
        	u_int32_t	debug;
        	u_int32_t	hostid;
        	char		ifname[IFNAMSIZ];
        	u_int8_t	pf_chksum[MD5_DIGEST_LENGTH];
        };

DIOCCLRSTATUS
    Clear the internal packet filter statistics.

DIOCNATLOOK struct pfioc_natlook *pnl
    Look up a state table entry by source and destination addresses and ports.

        struct pfioc_natlook {
        	struct pf_addr	 saddr;
        	struct pf_addr	 daddr;
        	struct pf_addr	 rsaddr;
        	struct pf_addr	 rdaddr;
        	u_int16_t	 sport;
        	u_int16_t	 dport;
        	u_int16_t	 rsport;
        	u_int16_t	 rdport;
        	sa_family_t	 af;
        	u_int8_t	 proto;
        	u_int8_t	 direction;
        };

DIOCSETDEBUG u_int32_t *level
    Set the debug level.

        enum	{ PF_DEBUG_NONE, PF_DEBUG_URGENT, PF_DEBUG_MISC,
        	  PF_DEBUG_NOISY };

DIOCGETSTATESV2 struct pfioc_states_v2 *ps
    Get state table entries.

        struct pfioc_states_v2 {
        	int		ps_len;
        	uint64_t	ps_req_version;
        	union {
        		void			*ps_buf;
        		struct pf_state_export	*ps_states;
        	};
        };
        struct pf_state_export {
        	uint64_t	 version;
        	uint64_t	 id;
        	char		 ifname[IFNAMSIZ];
        	char		 orig_ifname[IFNAMSIZ];
        	struct pf_state_key_export	 key[2];
        	struct pf_state_peer_export	 src;
        	struct pf_state_peer_export	 dst;
        	struct pf_addr	 rt_addr;
        	uint32_t	 rule;
        	uint32_t	 anchor;
        	uint32_t	 nat_rule;
        	uint32_t	 creation;
        	uint32_t	 expire;
        	uint32_t	 spare0;
        	uint64_t	 packets[2];
        	uint64_t	 bytes[2];
        	uint32_t	 creatorid;
        	uint32_t	 spare1;
        	sa_family_t	 af;
        	uint8_t		 proto;
        	uint8_t		 direction;
        	uint8_t		 log;
        	uint8_t		 state_flags_compat;
        	uint8_t		 timeout;
        	uint8_t		 sync_flags;
        	uint8_t		 updates;
        	uint16_t	 state_flags;
        	uint16_t	 qid;
        	uint16_t	 pqid;
        	uint16_t	 dnpipe;
        	uint16_t	 dnrpipe;
        	int32_t		 rtableid;
        	uint8_t		 min_ttl;
        	uint8_t		 set_tos;
        	uint16_t	 max_mss;
        	uint8_t		 set_prio[2];
        	uint8_t		 rt;
        	char		 rt_ifname[IFNAMSIZ];
        	uint8_t		 spare[72];
        };

DIOCCHANGERULE struct pfioc_rule *pcr
    Add or remove the rule in the ruleset specified by rule.action.

    The type of operation to be performed is indicated by action, which can be any of the following:

        enum	{ PF_CHANGE_NONE, PF_CHANGE_ADD_HEAD, PF_CHANGE_ADD_TAIL,
        	  PF_CHANGE_ADD_BEFORE, PF_CHANGE_ADD_AFTER,
        	  PF_CHANGE_REMOVE, PF_CHANGE_GET_TICKET };

    ticket must be set to the value obtained with PF_CHANGE_GET_TICKET for all actions except PF_CHANGE_GET_TICKET. pool_ticket must be set to the value obtained with the DIOCBEGINADDRS call for all actions except PF_CHANGE_REMOVE and PF_CHANGE_GET_TICKET. anchor indicates to which anchor the operation applies. nr indicates the rule number against which PF_CHANGE_ADD_BEFORE, PF_CHANGE_ADD_AFTER, or PF_CHANGE_REMOVE actions are applied.

DIOCCHANGEADDR struct pfioc_pooladdr *pca
    Add or remove the pool address addr from the rule specified by r_action, r_num, and anchor.

DIOCSETTIMEOUT struct pfioc_tm *pt

        struct pfioc_tm {
        	int		 timeout;
        	int		 seconds;
        };

    Set the state timeout of timeout to seconds. The old value will be placed into seconds. For possible values of timeout, consult the PFTM_* values in <net/pfvar.h>.

DIOCGETTIMEOUT struct pfioc_tm *pt
    Get the state timeout of timeout. The value will be placed into the seconds field.

DIOCCLRRULECTRS
    Clear per-rule statistics.

DIOCSETLIMIT struct pfioc_limit *pl
    Set the hard limits on the memory pools used by the packet filter.

        struct pfioc_limit {
        	int		index;
        	unsigned	limit;
        };
        enum	{ PF_LIMIT_STATES, PF_LIMIT_SRC_NODES, PF_LIMIT_FRAGS,
        	  PF_LIMIT_TABLE_ENTRIES, PF_LIMIT_MAX };

DIOCGETLIMIT struct pfioc_limit *pl
    Get the hard limit for the memory pool indicated by index.

DIOCRCLRTABLES struct pfioc_table *io
    Clear all tables. All the ioctls that manipulate radix tables use the same structure described below. For DIOCRCLRTABLES, pfrio_ndel contains on exit the number of tables deleted.

        struct pfioc_table {
        	struct pfr_table	 pfrio_table;
        	void			*pfrio_buffer;
        	int			 pfrio_esize;
        	int			 pfrio_size;
        	int			 pfrio_size2;
        	int			 pfrio_nadd;
        	int			 pfrio_ndel;
        	int			 pfrio_nchange;
        	int			 pfrio_flags;
        	u_int32_t		 pfrio_ticket;
        };
        #define pfrio_exists    pfrio_nadd
        #define pfrio_nzero     pfrio_nadd
        #define pfrio_nmatch    pfrio_nadd
        #define pfrio_naddr     pfrio_size2
        #define pfrio_setflag   pfrio_size2
        #define pfrio_clrflag   pfrio_nadd

DIOCRADDTABLES struct pfioc_table *io
    Create one or more tables. On entry, pfrio_buffer must point to an array of struct pfr_table containing at least pfrio_size elements. pfrio_esize must be the size of struct pfr_table. On exit, pfrio_nadd contains the number of tables effectively created.

        struct pfr_table {
        	char		pfrt_anchor[MAXPATHLEN];
        	char		pfrt_name[PF_TABLE_NAME_SIZE];
        	u_int32_t	pfrt_flags;
        	u_int8_t	pfrt_fback;
        };

DIOCRDELTABLES struct pfioc_table *io
    Delete one or more tables. On entry, pfrio_buffer must point to an array of struct pfr_table containing at least pfrio_size elements. pfrio_esize must be the size of struct pfr_table. On exit, pfrio_ndel contains the number of tables effectively deleted.

DIOCRGETTABLES struct pfioc_table *io
    Get the list of all tables. On entry, pfrio_buffer[pfrio_size] contains a valid writeable buffer for pfr_table structures. On exit, pfrio_size contains the number of tables written into the buffer. If the buffer is too small, the kernel does not store anything but just returns the required buffer size, without error.

DIOCRGETTSTATS struct pfioc_table *io
    This call is like DIOCRGETTABLES but is used to get an array of pfr_tstats structures.

        struct pfr_tstats {
        	struct pfr_table pfrts_t;
        	u_int64_t	 pfrts_packets
        			     [PFR_DIR_MAX][PFR_OP_TABLE_MAX];
        	u_int64_t	 pfrts_bytes
        			     [PFR_DIR_MAX][PFR_OP_TABLE_MAX];
        	u_int64_t	 pfrts_match;
        	u_int64_t	 pfrts_nomatch;
        	time_t		 pfrts_tzero;
        	int		 pfrts_cnt;
        	int		 pfrts_refcnt[PFR_REFCNT_MAX];
        };
        #define pfrts_name	 pfrts_t.pfrt_name
        #define pfrts_flags	 pfrts_t.pfrt_flags

DIOCRCLRTSTATS struct pfioc_table *io
    Clear the statistics of one or more tables. On entry, pfrio_buffer must point to an array of struct pfr_table containing at least pfrio_size elements. pfrio_esize must be the size of struct pfr_table. On exit, pfrio_nzero contains the number of tables effectively cleared.

DIOCRCLRADDRS struct pfioc_table *io
    Clear all addresses in a table. On entry, pfrio_table contains the table to clear. On exit, pfrio_ndel contains the number of addresses removed.

DIOCRADDADDRS struct pfioc_table *io
    Add one or more addresses to a table. On entry, pfrio_table contains the table ID and pfrio_buffer must point to an array of struct pfr_addr containing at least pfrio_size elements to add to the table. pfrio_esize must be the size of struct pfr_addr. On exit, pfrio_nadd contains the number of addresses effectively added.

        struct pfr_addr {
        	union {
        		struct in_addr	 _pfra_ip4addr;
        		struct in6_addr	 _pfra_ip6addr;
        	}		 pfra_u;
        	u_int8_t	 pfra_af;
        	u_int8_t	 pfra_net;
        	u_int8_t	 pfra_not;
        	u_int8_t	 pfra_fback;
        };
        #define pfra_ip4addr    pfra_u._pfra_ip4addr
        #define pfra_ip6addr    pfra_u._pfra_ip6addr

DIOCRDELADDRS struct pfioc_table *io
    Delete one or more addresses from a table. On entry, pfrio_table contains the table ID and pfrio_buffer must point to an array of struct pfr_addr containing at least pfrio_size elements to delete from the table. pfrio_esize must be the size of struct pfr_addr. On exit, pfrio_ndel contains the number of addresses effectively deleted.

DIOCRSETADDRS struct pfioc_table *io
    Replace the content of a table by a new address list. This is the most complicated command, which uses all the structure members.

    On entry, pfrio_table contains the table ID and pfrio_buffer must point to an array of struct pfr_addr containing at least pfrio_size elements which become the new contents of the table. pfrio_esize must be the size of struct pfr_addr. Additionally, if pfrio_size2 is non-zero, pfrio_buffer[pfrio_size..pfrio_size2] must be a writeable buffer, into which the kernel can copy the addresses that have been deleted during the replace operation. On exit, pfrio_ndel, pfrio_nadd, and pfrio_nchange contain the number of addresses deleted, added, and changed by the kernel. If pfrio_size2 was set on entry, pfrio_size2 will point to the size of the buffer used, exactly like DIOCRGETADDRS.

DIOCRGETADDRS struct pfioc_table *io
    Get all the addresses of a table. On entry, pfrio_table contains the table ID and pfrio_buffer[pfrio_size] contains a valid writeable buffer for pfr_addr structures. On exit, pfrio_size contains the number of addresses written into the buffer. If the buffer was too small, the kernel does not store anything but just returns the required buffer size, without returning an error.

DIOCRGETASTATS struct pfioc_table *io
    This call is like DIOCRGETADDRS but is used to get an array of pfr_astats structures.

        struct pfr_astats {
        	struct pfr_addr	 pfras_a;
        	u_int64_t	 pfras_packets
        			     [PFR_DIR_MAX][PFR_OP_ADDR_MAX];
        	u_int64_t	 pfras_bytes
        			     [PFR_DIR_MAX][PFR_OP_ADDR_MAX];
        	time_t		 pfras_tzero;
        };

DIOCRCLRASTATS struct pfioc_table *io
    Clear the statistics of one or more addresses. On entry, pfrio_table contains the table ID and pfrio_buffer must point to an array of struct pfr_addr containing at least pfrio_size elements to be cleared from the table. pfrio_esize must be the size of struct pfr_addr. On exit, pfrio_nzero contains the number of addresses effectively cleared.

DIOCRTSTADDRS struct pfioc_table *io
    Test if the given addresses match a table. On entry, pfrio_table contains the table ID and pfrio_buffer must point to an array of struct pfr_addr containing at least pfrio_size elements, each of which will be tested for a match in the table. pfrio_esize must be the size of struct pfr_addr. On exit, the kernel updates the pfr_addr array by setting the pfra_fback member appropriately.

DIOCRSETTFLAGS struct pfioc_table *io
    Change the PFR_TFLAG_CONST or PFR_TFLAG_PERSIST flags of a table. On entry, pfrio_buffer must point to an array of struct pfr_table containing at least pfrio_size elements. pfrio_esize must be the size of struct pfr_table. pfrio_setflag must contain the flags to add, while pfrio_clrflag must contain the flags to remove. On exit, pfrio_nchange and pfrio_ndel contain the number of tables altered or deleted by the kernel. Yes, tables can be deleted if one removes the PFR_TFLAG_PERSIST flag of an unreferenced table.

DIOCRINADEFINE struct pfioc_table *io
    Defines a table in the inactive set. On entry, pfrio_table contains the table ID and pfrio_buffer[pfrio_size] contains an array of pfr_addr structures to put in the table. A valid ticket must also be supplied to pfrio_ticket. On exit, pfrio_nadd contains 0 if the table was already defined in the inactive list or 1 if a new table has been created. pfrio_naddr contains the number of addresses effectively put in the table.

DIOCXBEGIN struct pfioc_trans *io

        struct pfioc_trans {
        	int		 size;	/* number of elements */
        	int		 esize;	/* size of each element in bytes */
        	struct pfioc_trans_e {
        		int		rs_num;
        		char		anchor[MAXPATHLEN];
        		u_int32_t	ticket;
        	}		*array;
        };

    Clear all the inactive rulesets specified in the pfioc_trans_e array. For each ruleset, a ticket is returned for subsequent "add rule" ioctls, as well as for the DIOCXCOMMIT and DIOCXROLLBACK calls.

    Ruleset types, identified by rs_num, include the following:

    PF_RULESET_SCRUB
        Scrub (packet normalization) rules.
    PF_RULESET_FILTER
        Filter rules.
    PF_RULESET_NAT
        NAT (Network Address Translation) rules.
    PF_RULESET_BINAT
        Bidirectional NAT rules.
    PF_RULESET_RDR
        Redirect rules.
    PF_RULESET_ALTQ
        ALTQ disciplines.
    PF_RULESET_TABLE
        Address tables.

DIOCXCOMMIT struct pfioc_trans *io
    Atomically switch a vector of inactive rulesets to the active rulesets. This call is implemented as a standard two-phase commit, which will either fail for all rulesets or completely succeed. All tickets need to be valid. This ioctl returns EBUSY if another process is concurrently updating some of the same rulesets.

DIOCXROLLBACK struct pfioc_trans *io
    Clean up the kernel by undoing all changes that have taken place on the inactive rulesets since the last DIOCXBEGIN. DIOCXROLLBACK will silently ignore rulesets for which the ticket is invalid.

DIOCSETHOSTID u_int32_t *hostid
    Set the host ID, which is used by pfsync(4) to identify which host created state table entries.

DIOCOSFPFLUSH
    Flush the passive OS fingerprint table.

DIOCOSFPADD struct pf_osfp_ioctl *io

        struct pf_osfp_ioctl {
        	struct pf_osfp_entry {
        		SLIST_ENTRY(pf_osfp_entry) fp_entry;
        		pf_osfp_t		fp_os;
        		char			fp_class_nm[PF_OSFP_LEN];
        		char			fp_version_nm[PF_OSFP_LEN];
        		char			fp_subtype_nm[PF_OSFP_LEN];
        	} 			fp_os;
        	pf_tcpopts_t		fp_tcpopts;
        	u_int16_t		fp_wsize;
        	u_int16_t		fp_psize;
        	u_int16_t		fp_mss;
        	u_int16_t		fp_flags;
        	u_int8_t		fp_optcnt;
        	u_int8_t		fp_wscale;
        	u_int8_t		fp_ttl;
        	int			fp_getnum;
        };

    Add a passive OS fingerprint to the table. Set fp_os.fp_os to the packed fingerprint, fp_os.fp_class_nm to the name of the class (Linux, Windows, etc), fp_os.fp_version_nm to the name of the version (NT, 95, 98), and fp_os.fp_subtype_nm to the name of the subtype or patchlevel. The members fp_mss, fp_wsize, fp_psize, fp_ttl, fp_optcnt, and fp_wscale are set to the TCP MSS, the TCP window size, the IP length, the IP TTL, the number of TCP options, and the TCP window scaling constant of the TCP SYN packet, respectively.

    The fp_flags member is filled according to the <net/pfvar.h> include file PF_OSFP_* defines. The fp_tcpopts member contains packed TCP options. Each option uses PF_OSFP_TCPOPT_BITS bits in the packed value. Options include any of PF_OSFP_TCPOPT_NOP, PF_OSFP_TCPOPT_SACK, PF_OSFP_TCPOPT_WSCALE, PF_OSFP_TCPOPT_MSS, or PF_OSFP_TCPOPT_TS.

    The fp_getnum member is not used with this ioctl.

    The structure's slack space must be zeroed for correct operation; memset(3) the whole structure to zero before filling and sending to the kernel.

DIOCOSFPGET struct pf_osfp_ioctl *io
    Get the passive OS fingerprint number fp_getnum from the kernel's fingerprint list. The rest of the structure members will come back filled. Get the whole list by repeatedly incrementing the fp_getnum number until the ioctl returns EBUSY.

DIOCGETSRCNODES struct pfioc_src_nodes *psn

        struct pfioc_src_nodes {
        	int	psn_len;
        	union {
        		caddr_t		psu_buf;
        		struct pf_src_node	*psu_src_nodes;
        	} psn_u;
        #define psn_buf		psn_u.psu_buf
        #define psn_src_nodes	psn_u.psu_src_nodes
        };

    Get the list of source nodes kept by sticky addresses and source tracking. The ioctl must be called once with psn_len set to 0. If the ioctl returns without error, psn_len will be set to the size of the buffer required to hold all the pf_src_node structures held in the table. A buffer of this size should then be allocated, and a pointer to this buffer placed in psn_buf. The ioctl must then be called again to fill this buffer with the actual source node data. After that call, psn_len will be set to the length of the buffer actually used.

DIOCCLRSRCNODES
    Clear the tree of source tracking nodes.

DIOCIGETIFACES struct pfioc_iface *io
    Get the list of interfaces and interface groups known to pf. All the ioctls that manipulate interfaces use the same structure described below:

        struct pfioc_iface {
        	char			 pfiio_name[IFNAMSIZ];
        	void			*pfiio_buffer;
        	int			 pfiio_esize;
        	int			 pfiio_size;
        	int			 pfiio_nzero;
        	int			 pfiio_flags;
        };

    If not empty, pfiio_name can be used to restrict the search to a specific interface or group. pfiio_buffer[pfiio_size] is the user-supplied buffer for returning the data. On entry, pfiio_size contains the number of pfi_kif entries that can fit into the buffer. The kernel will replace this value by the real number of entries it wants to return. pfiio_esize should be set to sizeof(struct pfi_kif).

    The data is returned in the pfi_kif structure described below:

        struct pfi_kif {
        	char				 pfik_name[IFNAMSIZ];
        	union {
        		RB_ENTRY(pfi_kif)	 pfik_tree;
        		LIST_ENTRY(pfi_kif)	 pfik_list;
        	};
        	u_int64_t			 pfik_packets[2][2][2];
        	u_int64_t			 pfik_bytes[2][2][2];
        	u_int32_t			 pfik_tzero;
        	u_int				 pfik_flags;
        	struct ifnet			*pfik_ifp;
        	struct ifg_group		*pfik_group;
        	u_int				 pfik_rulerefs;
        	TAILQ_HEAD(, pfi_dynaddr)	 pfik_dynaddrs;
        };

DIOCSETIFFLAG struct pfioc_iface *io
    Set the user settable flags (described above) of the pf internal interface description. The filtering process is the same as for DIOCIGETIFACES.

        #define PFI_IFLAG_SKIP	0x0100	/* skip filtering on interface */

DIOCCLRIFFLAG struct pfioc_iface *io
    Works as DIOCSETIFFLAG above but clears the flags.

DIOCKILLSRCNODES struct pfioc_iface *io
    Explicitly remove source tracking nodes.

FILES
/dev/pf
    packet filtering device.

EXAMPLES
The following example demonstrates how to use the DIOCNATLOOK command to find the internal host/port of a NATed connection:

    #include <sys/types.h>
    #include <sys/socket.h>
    #include <sys/ioctl.h>
    #include <sys/fcntl.h>
    #include <net/if.h>
    #include <netinet/in.h>
    #include <net/pfvar.h>
    #include <err.h>
    #include <stdio.h>
    #include <stdlib.h>
    u_int32_t
    read_address(const char *s)
    {
    	int a, b, c, d;
    	sscanf(s, "%i.%i.%i.%i", &a, &b, &c, &d);
    	return htonl(a << 24 | b << 16 | c << 8 | d);
    }
    void
    print_address(u_int32_t a)
    {
    	a = ntohl(a);
    	printf("%d.%d.%d.%d", a >> 24 & 255, a >> 16 & 255,
    	    a >> 8 & 255, a & 255);
    }
    int
    main(int argc, char *argv[])
    {
    	struct pfioc_natlook nl;
    	int dev;
    	if (argc != 5) {
    		printf("%s <gwy addr> <gwy port> <ext addr> <ext port>\n",
    		    argv[0]);
    		return 1;
    	}
    	dev = open("/dev/pf", O_RDWR);
    	if (dev == -1)
    		err(1, "open(\"/dev/pf\") failed");
    	memset(&nl, 0, sizeof(struct pfioc_natlook));
    	nl.saddr.v4.s_addr	= read_address(argv[1]);
    	nl.sport		= htons(atoi(argv[2]));
    	nl.daddr.v4.s_addr	= read_address(argv[3]);
    	nl.dport		= htons(atoi(argv[4]));
    	nl.af			= AF_INET;
    	nl.proto		= IPPROTO_TCP;
    	nl.direction		= PF_IN;
    	if (ioctl(dev, DIOCNATLOOK, &nl))
    		err(1, "DIOCNATLOOK");
    	printf("internal host ");
    	print_address(nl.rsaddr.v4.s_addr);
    	printf(":%u\n", ntohs(nl.rsport));
    	return 0;
    }

SEE ALSO
ioctl(2), altq(4), if_bridge(4), pflog(4), pfsync(4), pfctl(8), altq(9)

HISTORY
The pf packet filtering mechanism first appeared in OpenBSD 3.0 and then FreeBSD 5.2.

This implementation is derived from OpenBSD 4.5. A number of individual features, improvements, bug fixes and security fixes have been ported from later versions of OpenBSD. It has been heavily modified to be capable of running in multithreaded FreeBSD kernel and scale its performance on multiple CPUs.